SVGALINE drivers:

These drivers are based on the SVGALIB Linux library (at the time of 
writing version 1.9.11). The official SVGALIB site is www.svgalib.org.
The numbers in [] are the PCI device IDs of the video board models.
The numbers in () are the PCI vendor IDs of the video board manufacturers.

none	Disable the SVGALINE drivers

auto	Autodetect the correct video driver (default)

nv3	nVidia (10de), SGS (12d2)
	Riva 128 [0018]
	Riva TNT [0020], TNT2 [0028], Ultra TNT2 [0029], [002A], [002B], TNT2 (A) [002E], TNT2 (B) [002F]
	Riva Vanta [002C]
	Riva Ultra 64 [002D]
	Riva Integrated [00A0]
	GeForce 256 [0100], DDR [0101], Quadro [0103]
	GeForce2 MX [0110], MX DDR [0111], MXR [0113], GTS [0150,0151,0152], Quadro 2 Pro [0153]
	GeForce3 [0200,0201,0202,0203]

banshee	3dfx (121a) (interlaced mode not supported)
	Banshee [0003]
	Voodoo3 [0005]
	Voodoo5 [0009]

g400	Matrox (102b)
	Mystique [051a,051e]
	G100 [1000,1001]
	G200 [0520,0521]
	G400 [0525], G450 [0525]

millenium	Matrox (102b)
	Millenium 2064 [0519]
	Millenium II 2164 [051b,051f]

savage	S3 (5333)
	Trio 64 [8811], 3D [8903,8904], 3D 2X [8a13]
	Virge [5631], VX [883d], DX [8a01], GX2 [8a10], MX [8c00,8c01,8c02,8c03]
	Savage 3D [8a20,8a21], 4 [8a22,8a23], MX [8c10,8c12], 2000 [9102]

trident	Trident (1023)
	TGUI 9420DGi [9420], 9430DGi [9430], 9440AGi [9440,9460,9470], 96xx [9660]
	Cyber 9320 [9320], 9388 [9388], 9397 [9397], 939A/DVD [939A], 9520 [9520], 9525/DVD [9525], 9540 [9540]
	3DImage 975 [9750], 985 [9850]
	CyberBlade/i7 [8400], DSTN/i7 [8420], i1 [8500] DSTN/i1 [8520], Ai1 [8600], DSTN/Ai1 [8620], XP [9910], XPm [9930]
	Blade3D [9880]

r128	ATI (1002)
	Rage 128 PD [5044], PF [5046], PR [5052]
	Radeon QD [5144], QE [5145], QF [5146], QG [5147], VE [5159]
	Rage 128 RE [5245], RF [5246], RG [5247], RK [524B], RL [524C]
	Others [5000-54ff]

i740	Intel (8086)
	740 [00d1,7800]

i810	Intel (8086)
	810 [1132]

sis	SiS (1039)
	SG86C201 [0001], 202 [0002], 205 [0205], 215 [0215], 225 [0225]
	5597, 5598 [0200]
	300 [0300], 530 [6306], 540 [5300], 630 [6300]
	6326 [6326]

laguna	Cirrus (1013)
	Laguna 5462 [00d0]
	Laguna 5464 [00d4]
	Laguna 5465 [00d6]

apm	APM (1142)
	AT24 [6424]
	AT25/3D [643d]

rage	ATI (custom detection)
	Rage (many)

mx	MX (custom detection)
	86250, 86251

s3	S3 (custom detection)
	(many)

ark	ARK (custom detection)
	1000PV, 2000PV


VBELINE drivers:

These are the OLD drivers based on the VBE BIOS of the video board.
Some of them require the presence of an updated VBE BIOS like
the Scitech Display Doctor (shortly SDD).
These drivers are used only if none svgaline driver is detected.

none	Disable the VBELINE drivers

auto	Autodetect the correct video driver (default)

matrox	Matrox 
	Mystique 1064SG, G100, G200, G400

ati	ATI 
	Mach 64 (without SDD), ATI All-In-Wonder Pro (without SDD)

cirrus	Cirrus Logic (all with SDD)
	GD542?, GD5428, GD543? 

s3	S3 (with SDD)
	ViRGE, Vision 866, Vision 964, Trio32, Trio64, Trio64V+ 
	Aurora64V+, Trio64UV+, ViRGE/VX, 868, 928, 864, 964, 968, 
	Trio64 V2/DX, Trio64V2, ViRGE/DX, ViRGE/GX, ViRGE/GX2

s6326	SiS
	6326, 620, 530, 300, 630, 540

savage	S3 Savage
	Savage 3D, Savage 3DM, Savage 4

laguna	Cirrus Logic Laguna
	GD5462 Laguna, GD5464 Laguna, GD5465 Laguna

3dfx	3dfx (interlaced modes not supported)
	Banshee, Voodoo3, Voodoo5

r128	ATI Rage 128
	Rage 128 Mobility LE/LF/MF/ML, Rage 128 Pro PF/PR, 
	Rage 128 RE/RF/RK/RL, Rage 128 RF AGP, Rage 128 RK PCI
	Rage 128 RL AGP, 
	Rage 128 Pro (many), 
	Rage 128 (many)

neomagic	NeoMagic (interlaced modes not supported)
	MagicGraph 128 (NM2070), 128V (NM2090), 128ZV (NM2093)
	128ZV+ (NM2097), 128XD (NM2160)
	MagicMedia 256AV (NM2200), 256ZX (NM2360), 256XL+ (NM2380)

trident	Trident (without SDD)
	TGUI 9320, TGUI 9420, TGUI 9440, TGUI 9660
	Providia 9682, Providia 9685
	Cyber 9397, Cyber 9397/DVD, Cyber 9385, Cyber 9385-1
	Cyber 9382, Cyber 9388, Cyber 9397, Cyber 939A/DVD, Cyber 9520
	Cyber 9525/DVD, Cyber 9540
	3DImage975, 3DImage985
	CyberBlade/i7, CyberBlade/DSTN/i7, CyberBlade/i1, CyberBlade/DSTN/i1
	Blade3D, Blade3D/T64

vbe3	(interlaced modes rarely supported)
	Any video boards with a VBE3 BIOS which is also VGA compatible
	at registers level.
